HEATING CABLE
This particular kind of heating cable, extremely flexible and easily adaptable to complex shapes, can be used in many applications for its versatility.
It could be supplied in rolls or in single piece, according to the request of the customer, with related connections, connectors, wires, etc.
This type of cable can have integrated cold parts, avoiding any joins and, even, cold and heating sections also at different powers, along its whole length.
It is produced with resistive wire wounded around a fibre glass core and, according to the power and application, could be insulated by PVC or Silicone material.
Versions available: PVC or silicone cables covered by metal braid with single insulation (Class I) or double insulation (Class II).
